App(
    appid="flipperscope",
    name="[GPIO] Oscilloscope",
    fap_author="anfractuosity",
    apptype=FlipperAppType.EXTERNAL,
    entry_point="scope_main",
    requires=["gui"],
    stack_size=1 * 1024,
    fap_category="GPIO",
    fap_icon="scope_10px.png",
    fap_icon_assets="icons",
    fap_version="0.2",
    fap_description="Oscilloscope application - apply signal to pin 16/PC0, with a voltage ranging from 0V to 2.5V and ground to pin 18/GND",
)
