{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Лист1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист1","index":0,"n_rows":21,"n_cols":12,"rows_kept":21,"cut":false,"hidden":false,"merged":[[0,6,0,8],[0,9,0,11],[0,3,0,5],[0,0,1,0],[0,1,1,1],[0,2,1,2]]}
["Model","Power range","Interface","Temperature",null,null,"Humidity",null,null,"Pressure"]
[null,null,null,"Range","Accuracy","Resolution","Range","Accuracy","Resolution","Range","Accuracy","Resolution"]
["DHT11 (AOSONG)","3.3...5.5 V","Single wire","0...50 °C","±2 °C","1 °C","20...90 %","±5 %","1 %"]
["DHT11 (ASAIR)","3.3...5.5 V","Single wire","-20...60 °C","±2 °C","0.1 °C","5...95 %","±5 %","1 %"]
["DHT12","2.7...5.5 V","Single wire","-20...60 °C"," ±0.5 °C","0.1 °C","20...95 %","±5 %","0.1 %"]
["DHT21/AM2301","3.3...5 V","Single wire","-40...80 °C"," ±1 °C","0.1 °C","0...100%","±3 %","0.1 %"]
["DHT22/AM2302","3.3...5.5 V","Single wire","-40...80 °C"," ±0.5°C","0.1 °C","0...100%","±2%","0.1 %"]
["DHT20/AM2108","2.2...5.5 V","I2C","-40...80 °C"," ±0.5 °C","0.1 °C","0...100%","±3%","0.1 %"]
["AM2320","3.1...5.5 V","Single wire, I2C","-40...80 °C"," ±0.5 °C","0.1 °C","0...100%","±3%","0.1 %"]
["AHT10","1.8…3.6V","I2C","-40...85 °C"," ±0.3 °C","0.01 °C","0...100%","±2%","0.024 %"]
["AHT20","2…5.5V","I2C","-40...85 °C"," ±0.3 °C","0.01 °C","0...100%","±2%","0.024 %"]
["SHT30/GXHT30","2.2…5.5V","I2C","-40…125 °C"," ±0.3 °C","0.06 °C","0...100%","±3%","0.1 %"]
["SHT31/GXHT31","2.2…5.5V","I2C","-40…125 °C"," ±0.2 °C","0.06 °C","0...100%","±2%","0.1 %"]
["SHT35/GXHT35","2.2…5.5V","I2C","-40…125 °C"," ±0.1 °C","0.06 °C","0...100%","±1.5%","0.1 %"]
["LM75","2.8...5.5 V","I2C","-55...125°C","±2 °C","0.1 °C"]
["BMP180","1.8...3.6V","I2C","-40...85 °C","±0.5 °C","0.1 °C",null,null,null,"300...1100 hPA","±1.0 hPa","0.01 hPa"]
["BMP280","1.71...3.6 V","I2C","-40...85 °C","±0.5 °C","0.01 °C",null,null,null,"300...1100 hPA","±1.0 hPa","0.0016 hPa"]
["BME280","1.71...3.6 V","I2C","-40...85 °C","±0.5 °C","0.01 °C","0...100%","±3%","0.008%","300...1100 hPA","±1.0 hPa","0.0016 hPa"]
["DS18B20","3...5.5 V","One Wire","-55...125°C"," ±0.5 °C","0.1 °C"]
["DS18S20 (DS1820)","3...5.5 V","One Wire","-55...125°C"," ±0.5 °C","0.5 °C"]
["DS1822","3...5.5 V","One Wire","-55...125°C","±2 °C","0.1 °C"]