<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="17.45" y2="0" width="0.1524" layer="20"/>
<wire x1="17.45" y1="0" x2="17.45" y2="12.182" width="0.1524" layer="20"/>
<wire x1="17.45" y1="12.182" x2="0" y2="12.182" width="0.1524" layer="20"/>
<wire x1="0" y1="12.182" x2="0" y2="0" width="0.1524" layer="20"/>
<text>1/26/17</text>
<text>AT</text>
</plain>
<libraries>
<library name="ataradov_mcu">
<description>Alex Taradov Library (MCUs)</description>
<packages>
<package name="SO-14">
<description>SO-14</description>
</package>
</packages>
</library>
<library name="ataradov_conn">
<description>Alex Taradov Library (Connectors)</description>
<packages>
<package name="PIN-TH">
</package>
</packages>
</library>
<library name="ataradov_rlc">
<description>Alex Taradov Library (R, L and C)</description>
<packages>
<package name="SMD0603">
</package>
</packages>
</library>
<library name="ataradov_vreg">
<description>Alex Taradov Library (Voltage Regulators)</description>
<packages>
<package name="SOT23-5">
<description>SOT23-5</description>
</package>
</packages>
</library>
<library name="con-cypressindustries">
<description>&lt;b&gt;Connectors from Cypress Industries&lt;/b&gt;&lt;p&gt;
www.cypressindustries.com&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="32005-201">
<description>&lt;b&gt;MINI USB-B R/A SMT W/ REAR&lt;/b&gt;&lt;p&gt;
Source: http://www.cypressindustries.com/pdf/32005-201.pdf</description>
</package>
</packages>
</library>
<library name="ataradov_misc">
<description>Alex Taradov Library (Miscellaneous stuff)</description>
<packages>
<package name="TP-1.27MM">
</package>
</packages>
</library>
<library name="ataradov_led">
<description>Alex Taradov Library (LEDs and other indication devices)</description>
<packages>
<package name="SMD0603">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC2" library="ataradov_mcu" package="SO-14" value="ATSAMD11C">
<attribute name="NAME"/>
</element>
<element name="J5" library="ataradov_conn" package="PIN-TH" value="SIO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="ataradov_conn" package="PIN-TH" value="SCK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="ataradov_conn" package="PIN-TH" value="RST">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="ataradov_conn" package="PIN-TH" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="ataradov_rlc" package="SMD0603" value="1uF"/>
<element name="C2" library="ataradov_rlc" package="SMD0603" value="1uF">
<attribute name="NAME"/>
</element>
<element name="R2" library="ataradov_rlc" package="SMD0603" value="330"/>
<element name="R3" library="ataradov_rlc" package="SMD0603" value="330"/>
<element name="R4" library="ataradov_rlc" package="SMD0603" value="330"/>
<element name="IC1" library="ataradov_vreg" package="SOT23-5" value="MIC5504-3.3">
<attribute name="NAME"/>
</element>
<element name="R5" library="ataradov_rlc" package="SMD0603" value="100K"/>
<element name="R6" library="ataradov_rlc" package="SMD0603" value="100K"/>
<element name="X1" library="con-cypressindustries" package="32005-201" value="MINI-USB-32005-201">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="R7" library="ataradov_rlc" package="SMD0603" value="330"/>
<element name="TP1" library="ataradov_misc" package="TP-1.27MM" value="SIO"/>
<element name="TP2" library="ataradov_misc" package="TP-1.27MM" value=""/>
<element name="TP3" library="ataradov_misc" package="TP-1.27MM" value=""/>
<element name="TP4" library="ataradov_misc" package="TP-1.27MM" value=""/>
<element name="LED1" library="ataradov_led" package="SMD0603" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="IC2" pad="11"/>
<contactref element="J8" pad="1"/>
<contactref element="X1" pad="5"/>
<contactref element="TP4" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC2" pad="9"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="IC2" pad="10"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="V_USB">
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="IC1" pad="5"/>
<contactref element="C2" pad="2"/>
<contactref element="IC2" pad="12"/>
<contactref element="R6" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="LED1" pad="1"/>
</signal>
<signal name="SWDIO">
<contactref element="IC2" pad="8"/>
<contactref element="TP1" pad="1"/>
</signal>
<signal name="PA02">
<contactref element="IC2" pad="13"/>
</signal>
<signal name="PA04">
<contactref element="IC2" pad="14"/>
</signal>
<signal name="SWCLK">
<contactref element="IC2" pad="7"/>
<contactref element="R6" pad="1"/>
<contactref element="TP2" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="IC2" pad="6"/>
<contactref element="R5" pad="1"/>
<contactref element="TP3" pad="1"/>
</signal>
<signal name="PA15">
<contactref element="IC2" pad="5"/>
</signal>
<signal name="PA14">
<contactref element="IC2" pad="4"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="PA09">
<contactref element="IC2" pad="3"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="PA08">
<contactref element="IC2" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="PA05">
<contactref element="IC2" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="2"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="2"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R4" pad="2"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="N$8">
</signal>
<signal name="N$6">
<contactref element="R7" pad="2"/>
<contactref element="LED1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
